Liftgate Lock Striker Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Open the liftgate and suitably support it.
2. Remove the screws (1).
3. Disconnect the cable (3).
4. Remove the liftgate lock striker (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the cable (3).
2. Install the liftgate lock striker (2) with the screws (1).

Tighten
Tighten the liftgate lock striker screws (2) to 22 N·m (16 ft lb).