Intake Air Temperature Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the intake air temperature (IAT) sensor connector (1).
3. Disconnect the IAT sensor (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the IAT sensor.

Tighten
Tighten the IAT sensor to 20-30 N·m (15-22 lb ft).

2. Install the IAT sensor connector.
3. Connect the negative battery cable.