Power Window Inoperative - Passenger Door. Chevrolet Joy 2008

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Window Systems Connector End Views Connector End View Reference: Moveable Window Schematics
1 | Did you review the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Verify that the inoperative passenger door power window fault is present. Do the passenger door power windows operate normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3

3

1. Disconnect the appropriate passenger window switch.
2. Turn ON the ignition, with the engine OFF.
3. Probe the power window voltage supply circuit of the appropriate passenger window switch with a test lamp that is connected to a good ground.

Does the test lamp illuminate?

Go to Step 4

Go to Step 6

4

1. Connect a test lamp between the power window master switch up signal circuit of the appropriate passenger window switch and the power window master switch down signal circuit of the appropriate passenger window switch.
2. Activate the driver window switch to the UP and DOWN positions.

Does the test lamp illuminate?

Go to Step 5

Go to Step 7

5

1. Connect the appropriate passenger window switch.
2. Disconnect the appropriate passenger window motor.
3. Connect a test lamp between the power window motor up control circuit of the appropriate passenger window motor and the power window motor down control circuit of the appropriate passenger window motor.
4. Activate the appropriate passenger window switch to the UP and DOWN positions.

Does the test lamp illuminate?

Go to Step 9

Go to Step 8

6 | Test the power window voltage supply circuit of the appropriate passenger window switch for an open or short to ground. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 10
7 | Test the power window master switch signal circuits of the appropriate passenger window switch for a short to voltage or an open. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 10
8 | Test the power window motor circuits of the appropriate passenger window motor for a short to voltage or an open. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 11
9 | Inspect for poor connections at the appropriate passenger window motor. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 12
10 | Inspect for poor connections at the driver window switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 13
11 | Inspect for poor connections at the appropriate passenger window switch. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 15 | Go to Step 14
12 | Replace the appropriate passenger window motor. Refer to Door Window Regulator Replacement . Did you complete the replacement? | Go to Step 15 | --
13 | Replace the driver window switch. Did you complete the replacement? | Go to Step 15 | --
14 | Replace the appropriate passenger window switch. Did you complete the replacement? | Go to Step 15 | --
15 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2