Door Opening Weatherstrip Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Mark the door opening weatherstrip edge by a soluble pen.
2. Take off the rocker trim panel partially (2).
3. Take off the lower center pillar trim panel partially (3).
4. Remove the door opening weatherstrip (1).

### Installation Procedure

1. Install the door opening weatherstrip to match the marking.
2. Install the rocker panel trim and the lower center pillar panel trim.