Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Power Steering Gear Bracket Bolt | 50-55 N·m | 36-41 lb ft
Power Steering Gear Pinion Dust Cover | 45-55 N·m | 33-41 lb ft
Power Steering Gear Pinion Nut | 40-50 N·m | 30-36 lb ft
Power Steering Gear Pressure Line Fitting | 21-35 N·m | 16-26 lb ft
Power Steering Gear Return Line Fitting | 21-35 N·m | 16-26 lb ft
Power Steering Pressure Line Clamp Nut | 7-9 N·m | 62-80 lb in
Power Steering Pressure Line Coupling | 36-50 N·m | 27-37 lb ft
Power Steering Pressure Switch | 17-23 N·m | 13-17 lb ft
Power Steering Pump Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Front Bracket Adjusting Bolt | 18-22 N·m | 13-16 lb ft
Power Steering Pump Front Bracket Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Pressure Line Fitting | 21-35 N·m | 16-26 lb ft
Power Steering Pump Pulley Nut | 55-69 N·m | 41-51 lb ft
Power Steering Pump Rear Bracket Adjusting Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Rear Bracket Lower Bolt | 20-24 N·m | 15-18 lb ft
Power Steering Pump Rear Bracket Upper Bolt | 35-45 N·m | 26-33 lb ft
Power Steering Return Line Clamp Nut | 7-9 N·m | 62-80 lb in