Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
5th/Reverse Gear Shift Shaft Bolt | 10-16 N·m | 7-12 lb ft
Back Up Light Switch Nut | 15-18 N·m | 11-13 lb ft
Counter Shaft 5th Gear Nut | 60-80 N·m | 44-59 lb ft
Crankshaft Position Sensor Bolt | 5-8 N·m | 44-70 lb in
Differential Ring Gear Bolt | 80-100 N·m | 59-74 lb ft
Engine Mounting Front Bracket Bolt - Cylinder Block Side | 35-41 N·m | 25-30 lb ft
Engine Mounting Front Damping Bush Bolt - Crossmember Side | 35-41 N·m | 25-30 lb ft
Engine Mounting Front Damping Bush Bolts - Crossmember Side | 45-55 N·m | 33-41 lb ft
Engine Mounting Front Damping Bush Bolt/Nut - Bracket Side | 68-83 N·m | 51-61 lb ft
Front Exhaust Pipe Nut - Exhaust Manifold Side/Muffler Side | 25-35 N·m | 18-25 lb ft
Gear Shift Control Case Bolt | 18-28 N·m | 13-21 lb ft
Gear Shift Lever Bolt | 4-7 N·m | 35-62 lb in
High Speed Shift Shaft Bolt | 10-16 N·m | 7-12 lb ft
Low Speed Shift Shaft Bolt | 10-16 N·m | 7-12 lb ft
Oil Drain Plug | 25-30 N·m | 18-22 lb ft
Oil Level Plug | 25-30 N·m | 18-22 lb ft
Radiator Lower Hose Bracket Bolts | 8-15 N·m | 70-132 lb in
Reverse Idle Gear Shaft Bolt | 18-28 N·m | 13-21 lb ft
Reverse Shift Lever Bolt | 18-28 N·m | 13-21 lb ft
Select Cable Nut - Shift Lever Side | 8-12 N·m | 71-106 lb in
Select Lever Bolt | 18-28 N·m | 13-21 lb ft
Shift Guide Bolt | 18-28 N·m | 13-21 lb ft
Shift Interlock Bolt | 18-28 N·m | 13-21 lb ft
Side Cover Bolt | 8-12 N·m | 71-106 lb in
Side Cover Plate Screw | 6-7 N·m | 53-62 lb in
Speedometer Driven Gear Bolt | 4-7 N·m | 35-62 lb in
Starter Motor Bolt | 18-28 N·m | 13-21 lb ft
Transaxle Case Bolt | 15-22 N·m | 11-16 lb ft
Transaxle Case - Left Cap Bolt | 8-12 N·m | 71-106 lb in
Transaxle Lower Bolt and Nut - Engine Side | 55-65 N·m | 41-48 lb ft
Transaxle Mounting Bolt - Body Side | 45-55 N·m | 33-41 lb ft
Transaxle Mounting Bolt and Nut - Transaxle Side | 55-65 N·m | 41-48 lb ft
Transaxle Under Cover Bolt | 35-55 N·m | 25-41 lb ft
Transaxle Upper Bolt - Engine Side | 55-65 N·m | 41-48 lb ft