Air Inlet Grille Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the wiper arm assembly. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grille screws after removing the upper cap (2).
3. Remove the lower retaining plastic clips (1).
4. Close the hood.
5. Lift up the air inlet grille (3).
6. Disconnect the front washer hose connector.
7. Remove the air inlet grille (1).
8. Remove the front washer hose connector (2).

### Installation Procedure

1. Connect the front washer hose connector.
2. Install the air inlet grille with the screws and the clips.
3. Install the wiper arm assembly. Refer to Windshield Wiper Arm Replacement .