Clutch Pedal Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the clutch cable. Refer to Clutch Cable Replacement .
2. Release the clutch pedal return spring (1).
3. Remove the clutch pedal nut (4).
4. Remove the clutch pedal (2).
5. Remove the bushing (3).
6. Remove the pedal return spring (1).

### Installation Procedure

1. Install the pedal return spring.
2. Install the bushings.
3. Install the clutch pedal.
4. Install the nut.
5. Fix the pedal return spring.
6. Connect the clutch cable. Refer to Clutch Cable Replacement .
7. Adjust the clutch cable. Refer to Clutch Assembly Adjustment .