Rack and Pinion Boot Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the outer tie rod end. Refer to Rack and Pinion Outer Tie Rod End Replacement.
3. Remove the tie rod lock nut.
4. Remove the boot outer clamp (2).
5. Cut and remove the boot wire clamp (1).
6. Coat the tie rod (1) with lubricant in order to ease removal of the boot.
7. Remove the boot (2).

### Installation procedure

1. Install the boot to the tie rod.
2. Install the boot outer clamp.
3. Install the boot wire clamp.
4. Install the lock nut to the tie rod.
5. Install the outer tie rod end. Refer to Rack and Pinion Outer Tie Rod End Replacement.
6. Lower the vehicle.