Intake Air Temperature Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Disconnect the intake air temperature (IAT) sensor connector (1).
3. Disconnect the IAT sensor.
4. Remove the IAT sensor (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the IAT sensor.

Tighten
Tighten the IAT sensor to 20-30 N·m (15-22 lb ft).

2. Connect the IAT sensor connector (1).
3. Connect the negative battery cable.