Blower Motor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the blower motor electrical connector.
3. Remove the screws that secure the motor to the heater/air distribution case.
4. Remove the motor and the seal from the heater/air distribution case by gently pulling the motor straight down and out.

### Installation Procedure

1. Install the blower motor and seal, with the shock mount pads, in the heater/air distribution case. Hold the blower motor in position.
2. Install the blower motor screws to secure the blower motor to the heater/air distribution case.
3. Connect the electrical connector.
4. Connect the negative battery cable.
5. Confirm that the blower motor operates properly.