Front Side Door Jamb Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door jamb switch screw (1).
3. Disconnect the door jamb switch electrical connector (3).
4. Remove the door jamb switch (2).

### Installation Procedure

1. Install the door jamb switch with the screw.
2. Connect the electrical connector.
3. Connect the negative battery cable.