Master Cylinder Reservoir Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

1. Remove the fluid level switch connector. Refer to Brake Proportion Valve Replacement .

Notice: To prevent damage, do not use force when removing the reservoir.

2. Drain the brake fluid.
3. Remove the screw (1).
4. Remove the fluid reservoir using a flathead screwdriver (2).
5. Remove the reservoir.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: Use only General Motors recommended brake fluid.

1. Install the reservoir with the screw.

Tighten
Tighten the screw to 4 N·m (35 lb ft).

2. Install the fluid level switch connector. Refer to Brake Proportion Valve Replacement .
3. Add brake fluid.
4. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .