Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Camshaft Position Sensor Bolts | 10-14 N·m | 89-124 lb in
Crankshaft Position (CKP) Sensor Retaining Bolt | 5-8 N·m | 44-71 lb in
Electric Exhaust Gas Recirculation (EEGR) Valve Retaining Bolts | 20-30 ohms | 15-22 lb ft
Electronic Ignition (EI) System Ignition Coil Retaining Bolts | 8-12 N·m | 71-106 lb in
Engine Control Module (ECM) Mounting Bolts | 6-8 N·m | 53-71 lb in
Engine Coolant Temperature (ECT) Sensor | 8-12 N·m | 71-106 lb in
Evaporative Emission Canister Protective Cover | 8 N·m | 71 lb in
Fuel Rail Retaining Bolts | 18-22 N·m | 13-16 lb ft
Fuel Tank Strap Retaining Nuts | 18-22 N·m | 13-16 lb ft
Heated Oxygen Sensor | 35-44 N·m | 26-33 lb ft
Intake Air Temperature (IAT) Sensor | 20-30 N·m | 15-22 lb ft
Knock Sensor Bolt | 15-25 N·m | 11-18 lb ft
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 8-12 N·m | 71-106 lb in
Oxygen Sensor | 35-44 N·m | 26-33 lb ft
Throttle Body Retaining Bolt | 9-12 N·m | 80-106 lb in