Control Arm Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front stabilizer shaft. Refer to Stabilizer Shaft Replacement .
2. Remove the stud bolt (1).
3. Separate the control arm (2) from the knuckle assembly.
4. Remove the bolt (1).
5. Remove the control arm from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the control arm and the bolt (2) to the vehicle.

Tighten
Tighten the control arm bolt to 63 N·m (47 lb ft).

2. Install the control arm to the knuckle assembly.
3. Install the stud bolt (1).

Tighten
Tighten the stud bolt to 60 N·m (44 lb ft).

4. Install the front stabilizer shaft. Refer to Stabilizer Shaft Replacement .