Seat Belt Indicator Circuit Malfunction. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
The fuse F1 is blown. | Replace the fuse F1.
The seat belt warning lamp wiring harness is open circuit or short circuit. | Repair the wiring harness.
The continuity between the 2 terminals at the switch side of the connector has failed. | Replace the seat belt switch.
The continuity between the terminal for the BLK wire and ground has failed. | Repair the open ground.
The warning lamp bulb in the instrument cluster is blown. | Replace the wiring lamp bulb.