Fuel Filter Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Notice: Refer to Fuel Pressure Notice in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pump Replacement .
2. Disconnect the inlet/outlet fuel lines by pushing the line connector lock and pulling off the hose of the fuel filter tube (1).
3. Remove the screw from the retaining clamp.
4. Remove the fuel filter (1).

### Installation Procedure

Notice: Refer to Methanol Fuel Notice in the Preface section.

1. Install the new fuel filter into the retaining clamp. Note the flow direction.
2. Connect the inlet/outlet lines. Secure the lines with the connector lock.
3. Install the fuel pump.
4. Perform a leak test of the fuel filter.