Air Conditioning Evaporator Hose Assembly Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
3. Loosen the evaporative pipe line nut.
4. Remove the evaporative hose assembly.

### Installation Procedure

1. Install the A/C evaporative pipe.
2. Tighten the evaporative pipe line nut.
3. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .

Notice: Refer to Fastener Notice in the Preface section.

4. Recharge the A/C system. Refer to Refrigerant Recovery and Recharging .

Tightening
Tighten the evaporative pipe nut to 14 N·m (124 lb in).