Drum Brake System Description and Operation. Chevrolet Joy 2008

For 1990-2009 cars

This drum brake assembly is a leading/trailing shoe design. Both brake shoes are held against the wheel cylinder pistons by the lower return spring and the fixed anchor plate near the lower return spring. When the brakes are applied, the wheel cylinder pistons move both shoes out to contact the drum. With forward wheel rotation, the forward brake shoe will wrap into the drum and become self-energized. With reverse wheel rotation, the rear brake shoe is self-energized. Force from the brake shoes is transferred to the anchor plate through the backing plate to the axle flange. Adjustment is automatic and occurs on any service brake application. Do not switch the position of shoes that have been in service, as this may render the self-adjustment feature inoperative and result in increased pedal travel.

• | Replace all the components included in the repair kits used to service this drum brake.

• | Do not use lubricated shop air on the brake parts, as damage to the rubber components may result.

• | If any hydraulic component is removed or disconnected, it may be necessary to bleed all or part of the braking system.

• | The torque values specified are for dry, unlubricated fasteners.

• | Perform service operations on a clean bench that is free from all mineral oil materials.