Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Anchor End Nut | 33 N·m | 24 lb ft
Band Servo Stem | 3 N·m | 27 lb in
Bracket (Converter Housing) | 44 N·m | 33 lb ft
Bracket (Terminal Coupler) | 44 N·m | 32 lb ft
Bracket (Transmission Case) | 13 N·m | 115 lb in
Control Valve Upper - Countrol Valve Lower (Bolt) | 8 N·m | 71 lb in
Control Valve Upper - Countrol Valve Lower (Nut) | 8 N·m | 71 lb in
converter Housing Bolts | 31 N·m | 23 lb ft
Drain Plug | 40 N·m | 30 lb ft
Gear Shift Control Lever Bolts | 5 N·m | 44 lb in
Ground Wire Retaining Bolt | 30 N·m | 22 lb ft
Manual Shift Lock Bolt | 7 N·m | 62 lb in
Manual Shift Lock Nut | 13 N·m | 10 lb ft
Oil Cooler | 35 N·m | 26 lb ft
Oil Filler Tube | 7 N·m | 62 lb in
Oil Filter | 8 N·m | 71 lb in
Oil Pan Bolts | 13 N·m | 10 lb ft
Oil Pump Retaining Bolts | 13 N·m | 10 lb ft
Oil Pump Cover - Oil Pump Housing | 9 N·m | 80 lb in
Oil Temperature Sensor | 8 N·m | 71 lb in
Parking Pawl Shaft Stopper Bolt | 5 N·m | 44 lb in
PNP Switch | 3 N·m | 28 lb in
Radiator Lower Hose Bracket Bolts | 12 N·m | 106 lb in
Select Cable Bracket | 19 N·m | 14 lb ft
Select Lever Switch | 3 N·m | 27 lb in
Shift Cable Nuts | 10 N·m | 89 lb in
Shift Solenoid A | 8 N·m | 71 lb in
Shift Solenoid B | 8 N·m | 71 lb in
Support Actuator | 27 N·m | 20 lb ft
Torque Converter Bolts | 19 N·m | 14 lb ft
Transaxle Lower Bolt and Nut | 60 N·m | 45 lb ft
Transaxle Mount Lower Bolts | 37 N·m | 27 lb ft
Transaxle Mounting Bracket Bolt | 60 N·m | 45 lb ft
Transaxle Mount Upper Bolts | 60 N·m | 45 lb ft
Transmission Case - Control Valve Assembly | 8 N·m | 71 lb in
Transmission Case - Converter Housing | 28 N·m | 21 lb ft
Transmission Case - Oil Pan | 13 N·m | 115 lb in
Transmission Case - Oil Pump Assembly | 13 N·m | 115 lb in
Transmission Control Module (TCM) | 6 N·m | 53 lb in
Turbine Sensor | 7 N·m | 62 lb in
Vehicle Speed Sensor Retaining Bolt | 7 N·m | 62 lb in