Tire and Wheel Balancing. Chevrolet Joy 2008

For 1990-2009 cars

Balance is the easiest procedure to perform and should be done first if the vibration occurs at high speeds, or if the tires or the wheels are replaced.

Use the following wheel balancing procedure:

1. Do not use the wheel weight over two at the inboard and the outboard flanges
2. The total weight of the wheel weights should not exceed the 100 grams (3.5 ounces).
3. Blanching the assemblies with factory aluminum wheels requires the use of special nylon-coated, clip-on wheel weights.