Power Mirror Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the outside rearview mirror cover from the outside rearview mirror.
3. Remove the screws (3).
4. Disconnect the electrical connector (2).
5. Remove the outside rearview mirror (1).

### Installation Procedure

1. Connect the outside rearview mirror.
2. Install the outside rearview mirror with the screws.
3. Install the outside rearview mirror cover.
4. Connect the negative battery cable.