Gearshift Control Lever Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the floor console. Refer to Front Floor Console Replacement .
2. Disconnect the shift control cable. Refer to Shift Cable Replacement .
3. Remove the bolts and the gear shift control lever assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the bolts and the gear shift control lever assembly.

Tighten
Tighten gear shift lever bolts to 5 N·m (44 lb in).

2. Connect the shift control cable. Refer to Shift Cable Replacement .
3. Install the floor console. Refer to Front Floor Console Replacement .