Air Conditioning (A/C) Refrigerant Pressure Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Release the connector lock and pull the air conditioning (A/C) dual pressure switch wire connector out.
4. Hold the line fitting boss with one wrench and remove the A/C dual pressure switch with another wrench.
5. Discard the O-ring seal.

### Installation Procedure

1. Install the new seal on the A/C dual pressure switch.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the A/C dual pressure switch.

Tighten
Tighten the A/C dual pressure switch to 7 N·m (62 lb in).

3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .