Radio Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel (I/P) outer trim cover from the I/P. Refer to Instrument Panel Outer Trim Cover Replacement .
3. Remove the screws (1) from the audio system.
4. Disconnect the electrical connector and the antenna cable (2).
5. Remove the audio system (3) from the I/P.

### Installation Procedure

1. Connect the electrical connector and the antenna cable.
2. Install the audio system with the screws.
3. Install the I/P outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement .
4. Connect the negative battery cable.