DTC 17. Chevrolet Joy 2008

For 1990-2009 cars

### Circuit Description

When the transmission fluid is cold, the sensor resistance is high, As the transmission fluid warms up, the sensor resistance decreases. This diagnostic monitors the ATF temperature sensor circuit. The circuit may be functional but not in the normal operating range. this diagnostic indicates stuck, erratic, intermittent, or skewed values, resulting in reduced system performance.

If the TCM detects an intermittent voltage or no voltage change in the ATF temperature sensor circuit, then DTC 17 sets.

### Conditions for Running the DTC

• | The system voltage is between 9.0-18.0 volts

• | Road test the vehicle. Refer to Road Test .

### Conditions for Setting the DTC

Automatic transmission oil temperature is out of range, short circuit to voltage or circuit interruption.

### Action Taken When the DTC Sets

• | The TCM illuminates the A/T warning lamp when the diagnostic runs and fails

• | The TCM defaults to 80°C (176°F) and lockup and 4th gear are prohibited

• | Line pressure control is set to full throttle

### Conditions for Clearing the MIL/DTC

The TCM turns Off the A/T warning lamp when the diagnostic runs and does not fail.

#### DTC 17

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Automatic Transmission

2

1. Ignition OFF.
2. Disconnect the shift solenoid connector.
3. Start the engine.
4. Using a DMM, measure resistance at the shift solenoid connector between terminals B6 and B8.

Is the resistance within the specified value?

0.17k-2.5kohms

Go to Step 3

Go to Step 4

3 | Using a DMM, measure voltage at the shift solenoid connector between terminals B6 and B8. Is the voltage within the specified value? | 2-3 volt | Go to Step 6 | Go to Step 5
4 | Replace the ATF temperature sensor circuits for an open, short to voltage or short to ground. Did you complete the replacement? | -- | Go to Step 7 | --
5 | Inspect the ATF temperature sensor circuits for an open, short to voltage or short to ground. Did you find and correct the condition? | -- | Go to Step 7 | Go to Step 6
6 | Replace the TCM. Refer to Transmission Control Module Replacement . Did you complete the replacement? | -- | Go to Step 7 | --

7

1. Clear the DTCs. Refer to Clearing Transmission Diagnostic Trouble Codes .
2. Start the engine.
3. Operate the vehicle within Conditions for Running the DTC.

Does the DTC reset?

--

Go to Step 2

System OK