Turn Signal Multifunction Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the steering column covers. Refer to Steering Column Trim Covers Replacement .
3. Disconnect the turn signal switch by pushing the tabs (1) on the switch housing.
4. Disconnect the connectors (2).
5. Remove the turn signal switch.
6. Disconnect the wiper switch by pushing tabs (1) on the switch housing.
7. Disconnect the connectors (2).
8. Remove the wiper switch.

### Installation Procedure

1. Install the wiper switch.
2. Connect the connectors.
3. Install the turn signal switch.
4. Connect the connectors.
5. Install the steering column covers. Refer to Steering Column Trim Covers Replacement .
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .