Brake Pedal Assembly Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
2. Remove the stop lamp switch. Refer to Stop Lamp Switch Replacement .
3. Remove and discard the cotter pin (1).
4. Remove the clevis pin (2).
5. Remove the brake pedal nut and the brake pedal bolt (1).
6. Remove the brake pedal spring (2).
7. Remove the bushings (1).
8. Remove the brake pedal pad (3).
9. Remove the brake pedal.

### Installation Procedure

1. Install the brake pedal pad (3).
2. Install the bushings (1).
3. Install the brake pedal spring (2).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the brake pedal to the pedal bracket with a bolt (1) and a nut.

Tighten
Tighten the bolt and the nut to 18 N·m (13 lb ft).

5. Install the clevis pin (2).
6. Install a NEW cotter pin (1).
7. Install the stop lamp switch. Refer to Stop Lamp Switch Replacement .
8. Install the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .