Tail Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the tailgate.
3. Remove the tail lamp screws.
4. Disconnect the electrical connector.
5. Remove the tail lamp assembly.

### Installation Procedure

1. Install the tail lamp assembly with the screws.
2. Connect the electrical connector.
3. Close the tailgate.
4. Connect the negative battery cable.