Defroster Grille Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
3. Remove the screws and the defroster grille.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the defroster grille to the instrument panel with the screws.

Tighten
Tighten the screws to 3 N·m (27 in lb).

2. Install the instrument cluster. Refer to Instrument Cluster Replacement .
3. Connect the negative battery cable.