Instrument Panel Carrier Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
3. Remove the defroster duct hose from the tie-bar.
4. Remove the steering column. Refer to Steering Column Replacement .
5. Remove the electrical wiring harness strip.
6. Disconnect the electrical wiring harness.
7. Remove the defroster duct.
8. Remove the bolts and the tie-bar.
9. Remove the bolts and the tie-bar center.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tie-bar with the bolts.

Tighten
Tighten the bolts to 13 N·m (115 in lb).

2. Install the tie-bar center with the bolts.

Tighten
Tighten the bolts to 13 N·m (115 in lb).

3. Install the defroster duct to the upper air inlet grille panel.
4. Connect the electrical wiring harness.
5. Bind the electrical wiring harness strip.
6. Install the steering column. Refer to Steering Column Replacement .
7. Install the defroster duct hose.
8. Install the instrument panel assembly. Refer to Instrument Panel Assembly Replacement .
9. Connect the negative battery cable.