Manual Shift Detent Lever with Shaft Position Switch Assembly and Park Pawl Actuator Installation. Chevrolet Nubira (Delta) 2010

For 1990-2009 cars

Table 1: | Park Pawl and Actuator Guide Installation
Table 2: | Installation

### Park Pawl Actuator Guide Installation

#### Park Pawl and Actuator Guide Installation

Callout | Component Name
--- | ---
1 | Park Pawl Actuator Guide Assembly Seal
2 | Park Pawl Actuator Guide Assembly

3

Park Pawl Actuator Guide Pin

#### Procedure

Install the Park Pawl Actuator Guide Pin to correct height.

Specification:
9.7 mm (0.38 in)

### Installation

Callout | Component Name
--- | ---
1 | Park Pawl Actuator Assembly
2 | Manual Shift Detent (w/Shaft Position Switch) Lever Assembly
3 | Manual Shaft Tip Lubricate the shaft with ATF to prevent damage to the manual shift shaft seal during installation.

4

Manual Shaft Detent Lever Hub Pin

Tip
Use a NEW pin to ensure proper engagement with the shaft. DT-48550 can also be used to install the pin.

#### Procedure

Install the Manual Shaft Detent Lever Hub Pin to correct height.

Specification:
(b) 7.9 mm (0.38 in)

#### Special Tool

DT-48550 Detent Lever Pin Remover

For equivalent regional tools, refer to Special Tools.

5

Manual Shift Shaft Pin

Caution: Use J 41229 to install the manual shaft pin at the correct height in order to properly secure the manual shaft. If you install the pin too deep, the case bore may crack.

Tip
Use a NEW pin to ensure proper engagement with the case.

#### Procedure

Inspect pin installed height is within (a).

Specification:
(a) 7.2-8.2 mm (0.28-0.32 in)

#### Special Tool

DT-41229 Manual Shaft Pin Installer

For equivalent regional tools, refer to Special Tools.