Transmission Fluid Pump, Front Differential Carrier Baffle, and Front Differential Ring Gear Installation. Chevrolet Nubira (Delta) 2010

For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter and Differential Housing Seal
2 | Fluid Pump Assembly

3

Fluid Pump Bolts M8 x 33 (Qty: 8)

Caution: Refer to Fastener Caution in the Preface section.

Tighten
10 N·m (89 lb in) then rotate the bolt an additional 45 degrees

#### Special Tool

EN-45059 Angle Meter or equivalent

For equivalent regional tools, refer to Special Tools.

4 | Front Differential Ring Gear
5 | Front Differential Ring Gear Retainer Tip Install the retainer with the taper facing away from the ring gear.
6 | Front Differential Carrier Baffle
7 | Front Differential Carrier Baffle Bolts M6 x 25 (Qty: 2) Tighten 12 N·m (106.21 lb in)