Converter Housing Installation. GMC Truck Export Savana 1999

For 1990-2009 cars

#### Tools Required

J 41510 50 mm Torx® Plus Bit

1. Install the converter housing (102).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the converter housing bolts (94) to the transmission case. Use the J 41510 .

Tighten
Tighten the converter housing bolts (94) to 65-75 N·m (48-55 lb ft).