Low and Reverse Band Servo Assembly Removal. GMC Truck Export GMC P42 Commercial Chassis 2000

For 1990-2009 cars

1. Remove the low and reverse band servo cover bolts (61).
2. Remove the low and reverse band servo cover (62).
3. Remove the low and reverse band servo cover gasket (63).
4. Inspect the low and reverse band servo cover (62) for damage.
5. Remove the low and reverse band servo assembly (64-73).
6. Remove the low and reverse accumulator piston spring (74) from the transmission case.
7. Inspect the low and reverse band servo transmission case bore for wear and scoring.
8. Inspect the low and reverse accumulator piston spring (74) for distortion.