4th Clutch Plate Installation. GMC Truck Export GMC P42 Commercial Chassis 2000

For 1990-2009 cars

Note: Alternate the fourth clutch plates (525, 526), starting with a steel clutch plate (526) (4 steel, 4 composite). Install the fourth clutch steel plates (526) with the V notch tang at the 1 o'clock position in the fourth clutch housing.

1. Install the fourth clutch plates (525, 526) into the fourth clutch housing (529).
2. Install the fourth clutch backing plate (524). Align the notched tab of the fourth clutch backing plate (524) over the anchor pin in the case.
3. Install the fourth clutch backing plate retainer ring (523).