GEAR RATTLE IN NEUTRAL SERVICE REPAIR/CLUTCH. GMC Truck S15 Pickup - 2WD 1982

For 1990-2009 cars

# GEAR RATTLE IN NEUTRAL SERVICE REPAIR/CLUTCH

MANUAL TRANSMISSION GEAR RATTLE IN THE 1982 "S" TRUCKS EQUIPPED WITH V6 ENGINES THAT ARE DATE STAMPED PRIOR TO T1007 CAN BE IMPROVED BY THE INSTALLATION OF A NEW CLUTCH DRIVEN DISC, P/N 14054858. THE DATE STAMP IS LOCATED ON THE ENGINE BLOCK DECK NEXT TO THE NUMBER TWO (2) CYLINDER JUST REAR OF THE WATER PUMP.

NOTE; A REVISED BULLETIN IS IN PROCESS. SEE T148 FOR ADDITIONAL PART NUMBERS AND INFORMATION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.