CAMPAIGN: WINDSHIELD AND STATIONARY GLASS RETENTION. GMC Truck S15 Pickup - 2WD 1991

For 1990-2009 cars

# CAMPAIGN: WINDSHIELD AND STATIONARY GLASS RETENTION

CAMPAIGN NUMBER: 91C01 GROUP: 10A3 - GLASS

#### SUBJECT: WINDSHIELD/STATIONARY SIDE GLASS RETENTION

#### MODELS: 1991 S/T UTILITY/PICKUP/BLAZER/EXTENDED CAB PICKUP

** SEE BOTTOM OF CAMPAIGN FOR INFORMATION CONCERNING OTHER AFFECTED ** DIVISIONS.

DEFECT INVOLVED

GENERAL MOTORS HAS DETERMINED THAT CERTAIN 1991 S/T UTILITY/PICKUP/ EXTENDED CAB PICKUPS MAY FAIL TO CONFORM TO THE REQUIREMENTS OF FEDERAL MOTOR VEHICLE SAFETY STANDARD FMVSS 212"WINDSHIELD MOUNTING"

THESE VEHICLES MAY EXHIBIT POOR BOND ADHESION BETWEEN THE WINDSHIELD GLASS AND MOUNTING, WHICH COULD ALLOW THE WINDSHIELD TO SEPARATE FROM THE VEHICLE DURING A COLLISION. SHOULD WINDSHIELD SEPARATION OCCUR DURING A COLLISION, AN UNBELTED OCCUPANT COULD BE EJECTED FROM THE VEHICLE AND PERSONAL INJURY COULD OCCUR.

IN ADDITION TO THE WINDSHIELD RETENTION, IT HAS ALSO BEEN DETERMINED THAT A CUSTOMER SATISFACTION ISSUE MAY BE PRESENT REGARDING THE RETENTION OF THE STATIONARY SIDE WINDOWS (S/T UTILITY/EXTENDED CAB PICKUPS WITH NON-MOVEABLE SIDE WINDOWS).

BOTH OF THE ABOVE CONDITIONS WERE CAUSED BY IMPROPER PRIMER HAVING BEEN INSTALLED ON THE METAL SURFACE OF THE SIDE WINDOW AND WINDSHIELD OPENING, RESULTING IN LOW ADHESION TO THE METAL SURFACE. RESULTING IN LOW ADHESION TO THE METAL SURFACE.

TO CORRECT THIS CONDITION IT WILL BE NECESSARY TO REMOVE AND REINSTALL THE WINDSHIELD AND STATIONARY GLASS QUARTER WINDOWS ACCORDING TO THE INSTRUCTIONS DESCRIBED IN THIS COMMUNICATION.

THIS REPAIR MUST BE PERFORMED PRIOR TO VEHICLE SALE.

THIS BULLETIN IS NOTICE TO YOU THAT THE NEW MOTOR VEHICLES INCLUDED IN THIS CAMPAIGN MAY NOT COMPLY WITH THE STANDARD IDENTIFIED ABOVE. UNDER SECTION 108 OF THE NATIONAL TRAFFIC AND MOTOR VEHICLE SAFETY ACT, IT IS ILLEGAL FOR A DEALER TO SELL A NEW MOTOR VEHICLE WHICH THE DEALER KNOWS DOES NOT COMPLY WITH AN APPLICABLE FEDERAL MOTOR VEHICLE SAFETY STANDARD. AS A CONSEQUENCE, IF YOU SELL ANY OF THESE MOTOR VEHICLES WITHOUT FIRST PERFORMING THE COMPAIGN CORRECTION, YOUR DEALERSHIP MAY BE SUBJECT TO A CIVIL PENALTY UP TO $1,000 FOR EACH SALE.

VEHICLES INVOLVED

INVOLVED ARE CERTAIN 1991 S/T UTILITY/PICKUPS BUILT AT THE MORAINE ASSEMBLY PLANT. VIN'S AND DEALER CODES ARE LISTED BELOW:

GMC VEHICLES

48-42307 1GTCS14E6M2504209 48-51227 1GTCS14E6M2504274 48-10390 1GTCS14Z9M2504210 48-40220 1GTCS14E2M2504286 48-44590 1GTCT14Z5M2504220 48-53519 1GTCS14Z4M2504289 48-21022 1GTCS19Z4M2504222 48-42296 1GTCS14Z0M2504290 48-50368 1GTCS19Z8M2504224 48-30427 1GTCS14E8M2504292 48-40060 1GTDT14Z9M2504225 48-40001 1GTCS14Z6M2504293 48-42236 1GTCS14Z1M2504234 48-21725 1GTCS14E1M2504294 48-53191 1GTCS14E2M2504238 48-40220 1GTCS14E3M2504295 48-21734 1GTDT19Z8M2504239 48-51227 1GTCS14E6M2504303 48-42067 1GTCS14Z9M2504241 48-44030 1GTCS19R3M2504311 48-42038 1GTCS19ZXM2504242 48-50265 1GTCS14E7M2504316 48-50368 1GTCS14Z2M2504243 48-21041 1GTCS19Z1M2504324 48-50486 1GTCS14Z6M2504245 48-21350 1GTCS14E3M2504228 48-51220 1GTCS14E3M2504247 48-50184 1GTCS14ZXM2504331 48-50184 1GTCS19Z0M2504251 48-51227 1GTCS14EXM2504343 48-50505 1GTCS14Z3M2504266 48-30860 1GTCS14Z9M2504353 48-42313 1GTCS19Z4M2504270 48-53068 1GTCS14EXM2504357 48-50368 1GTCS19ZXM2504273

NO OWNER LETTER WILL BE SENT SINCE THE VEHICLES SHOULD STILL BE IN YOUR NEW VEHICLE INVENTORY. IF ANY HAVE BEEN DELIVERED, PLEASE IMMEADIATELY CONTACT THE OWNER AND PERFORM THIS MODIFICATION.

#### SERVICE INFORMATION:

#### MODEL REMOVAL REQUIRED 1991 S/T SERVICE MANUAL X-9129 ----- ---------------- ------------------------------

PICKUP WINDSHIELD PAGE 10A3-2, FIG. 1 # 306

EXTENDED CAB WINDSHIELD PAGE 10A3-2, FIG. 1 # 306 PICKUP WITH MOVEABLE SIDE WINDOWS

EXTENDED CAB WINDSHIELD, PAGE 10A3-2, FIG. 1 # 306 PICKUP WITH STATIONARY SIDE PAGE 10A3-8, FIG. 1 # 334 STATIONARY SIDE WINDOWS WINDOWS

JIMMY (UTILITY) WINDSHIELD PAGE 10A3-2, FIG. 1 # 306 STATIONARY PAGE 10A3-6, FIG. 14 # 315 SIDE WINDOWS

WINDSHIELDS AND STATIONARY GLASS REAR QUARTER WINDOWS SHOULD BE REMOVED AND REINSTALLED USING PROCEDURES OUTLINED IN THE 1991 S/T SERVICE MANUAL X-9129, SECTION 10A3.

AFTER WINDSHIELD AND QUARTER WINDOW REMOVAL, THE METAL SURFACE OF THE WINDOW OPENING MUST HAVE THE BLACK PRIMER (INCORRECT) REMOVED COMPLETELY. THIS MAY BE ACCOMPLISHED BY APPLYING DUCT TAPE TO THE PRIMED SURFACE AND THEN QUICKLY STRIPPING THE TAPE FROM THE VEHICLE. THE MAJORITY OF THE PRIMER WILL ADHERE TO THE TAPE. THE PRIMER THAT REMAINS ADHERED TO THE BODY SHOULD BE REMOVED USING NAPTHA.

THE WINDOW OPENING SHOULD THEN BE REPRIMED WITH THE #3 METAL PRIMER PROVIDED IN THE FURNISHED KIT. THE GLASS SHOULD BE REINSTALLED FOL- LOWING THE INSTALLATION PROCEDURE OUTLINED IN SECTION 10A3, USING THE #1 GLASS PREP AND #2 GLASS PRIMER FURNISHED.

IF THIS REPAIR IS SUBLET TO A GLASS REPLACEMENT FACILITY PROVIDE THIS FACILITY WITH THE REQUIRED INSTALLATION PROCEDURE, A COPY OF THIS NOTIFICATION AND THE FURNISHED INSTALLATION KIT(S).

PARTS INFORMATION

THE REQUIRED NUMBER OF INSTALLATION KITS WILL BE SHIPPED TO INVOLVED DEALERS BY GMC TRUCK ON A NO CHARGE BASIS.

IF ADDITIONAL KITS ARE REQUIRED, THEY MAY BE OBTAINED BY CONTACTING ADISTRA CORPORATION (313) 455-9072. VIN WILL BE REQUIRED WHEN ORDER- ING ADDITIONAL KITS.

DO NOT ORDER KITS FROM GENERAL MOTORS SERVICE PARTS OPERATION (GMSPO)

THE INSTALLATION KITS CONTAIN:

KIT A 1- WINDSHIELD REVEAL MOLDING 1- URETHANE 1- GLASS PREP #1 1- GLASS PRIMER #2 1- METAL PRIMER #3

KIT B 1- URETHANE 1- GLASS PREP #1 1- GLASS PRIMER #2 1- METAL PRIMER #3

ON STANDARD PICKUP AND EXTENDED CAN PICKUPS WITH MOVEABLE SIDE QUARTER WINDOWS, ONE (1) "A" KIT WILL BE FURNISHED.

ON JIMMY (UTILITY) AND EXTENDED CAB PICKUPS WITH STATIONARY QUARTER WINDOWS, THREE (3) INSTALLATION KITS (1 "A" KIT AND 2 "B" KITS) WILL BE FURNISHED.

WARRANTY INFORMATION

DEALERS SHOULD SUBMIT AN ACCURATELY FILLED OUT WARRANTY REPAIR ORDER ON EACH VEHICLE COMPLETED UNDER THIS CAMPAIGN.

LABOR OPERATION *TIME **PARTS TROUBLE NUMBER DESCRIPTION ALLOWANCE ALLOWANCE CODE

V6010 PICKUP 1.3 HRS $ 8.48 96

V6011 EXTENDED CAB 1.3 HRS $ 8.48 96 PICKUP WITH MOVEABLE QUARTER WINDOWS

V6012 EXTENDED CAB 2.3 HRS $ 21.78 96 PICKUP WITH STATIONARY SIDE WINDOWS

V6013 JIMMY (UTILITY) 3.1 HRS $ 21.78 96 WITH STATIONARY SIDE WINDOWS

* FOR DEALER TO RECEIVE ADMINISTRATIVE TIME ALLOWANCE ASSOCIATED WITH THIS CAMPAIGN, ADD 0.1 HOUR TO THE LABOR OPERATION TIME ALLOWANCE.

** THE AMOUNTS IDENTIFIED IN THE "PARTS ALLOWANCE" COLUMN ABOVE REPRESENT 30% OF DEALER NET FOR PARTS THAT WERE FURNISHED BY GMC TRUCK DIVISION. THIS AMOUNT IS TO BE PLACED IN THE NET ITEM AMOUNT COLUMN OF THE CLAIM AND USE TYPE CODE "M".

CAMPAIGN IDENTIFICATION LABEL

EACH VEHICLE CORRECTED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS CAMPAIGN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL". EACH LABEL PROVIDES A SPACE TO INCLUDE THE CAMPAIGN NUMBER AND THE FIVE (5) DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR BALL POINT PEN.

EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN FOR PERIODIC SERVICING BY THE OWNER.

APPLY "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN, DRY SURFACE.

ADMINISTRATIVE PROCEDURE

PROCEDURES COVERING THIS CAMPAIGN ARE OUTLINED IN SECTION V OF YOUR DEALERSHIP'S "GM TRUCK CLAIMS PROCESSING MANUAL" #P8919.

** CHEVROLET ONLY INFORMATION:

VEHICLES INVOLVED FOR CHEVROLET ONLY

YEAR MODEL PLANT FROM THROUGH 1991 S/T MORAINE M2119115 M2119682

INVOLVED ARE CERTAIN 1991 CHEVROLET S/T TRUCKS (BLAZER/PICKUP/ EXTENDED CAB PICKUP) BUILD WITHIN THE ABOVE VIN BREAKPOINTS: INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER COMPUTER LISTINGS.

#### SERVICE PROCEDURE:

1. REMOVE WINDSHIELD AND STATIONARY GLASS REAR QUARTER WINDOWS USING PROCEDURES OUTLINDED IN THE 1991 S/T SERVICE MANUAL ST369-91, SECTION 10A3. WINDOW REMOVAL NECESSARY FOR EACH VEHICLE TYPE AND THE APPLICABLE SERVICE MANUAL PAGES ARE SHOWN IN THE FOLLOWING CHARTS. 1991 S/T SERVICE MODEL REMOVAL REQUIRED MANUAL ST 369-91 ----------- --------------------- --------------------- PICKUP WINDSHIELD PAGE 10A3-2, FIG. 1 #306

EXTENDED CAB WINDSHIELD PAGE 10A3-2, FIG. 1 #306 PICKUP WITH MOVEABLE SIDE WINDOWS

EXTENDED CAB WINDSHIELD AND PAGE 10A3-2, FIG. 1 #306 PICKUP WITH STATIONARY SIDE STATIONARY WINDOWS PAGE 10A3-8, FIG. 17 #334 SIDE WINDOWS

BLAZER (UTILITY) WINDSHIELD AND PAGE 10A3-2, FIG. 1 #306 STATIONARY SIDE WINDOWS PAGE 10A3-6, FIG. 14 #315

2. AFTER REMOVING WINDSHIELD AND QUARTER WINDOWS (AS NECESSARY), THE METAL SURFACE OF THE WINDOW OPENING MUST HAVE THE BLACK PRIMER (INCORRECT) REMOVED COMPLETELY. THIS MAY BE ACCOMPLISHED BY APPLYING DUCT TAPE TO THE PRIMED SURFACE AND THEN QUICKLY STRIPPING TAPE FROM THE VEHICLE. THE MAJORITY OF THE PRIMER WILL ADHERE TO THE TAPE. THE PRIMER THAT REMAINS ADHERED TO THE BODY SHOULD THEN BE REMOVED USING NAPTHA.

3. REPRIME THE WINDOW OPENING WITH #3 METAL PRIMER PROVIDED IN THE APPLICABLE KIT.

4. REINSTALL THE GLASS FOLLOWING THE PROCEDURE OUTLINED IN MANUAL SECTION 10A3 (SEE CHART ABOVE FOR APPLICABLE PAGE NUMBER). USE THE #1 GLASS PREP AND #2 GLASS PRIMER FURNISHED IN THE APPROPRIATE KIT AS REQUIRED BY MANUAL INSTRUCTIONS.

5. INSTALL CAMPAIGN IDENTIFICATION LABLE.

#### NOTICE: IF THIS REPAIR IS SUBLET TO A GLASS REPLACEMENT FACILITY, PROVIDE THIS FACILITY WITH THE REQUIRED INSTALLATION PROCEDURE, A COPY OF THIS NOTICICATION AND THE FURNISHED INSTALLATION KIT(S).

CHEVROLET CLAIM INFORMATION: * ** FAILED PARTS CC LB LB OTH NET REPAIR PERFORMED PC PART NO. ALLOW FC OP HR HRS AMT ---------------- -- -------- ----- -- -- --- --- --- REINSTALL GLASS- - - - - - SK V6010 1.3 0.1 $8.48 PICKUP 00

REINSTALL GLASS- - - - - - SK V6011 1.3 0.1 $8.48 EXTENDED CAB WITH 00 MOVABLE QUARTER REAR WINDOWS

REINSTALL GLASS- - - - - - SK V6012 2.3 0.1 $21.78 EXTENDED CAB WITH 00 STATION SIDE WINDOWS

REINSTALL GLASS - - - - - SK V6013 3.1 0.1 $21.78 BLAZER (UTILITY) 00

* CAMPAIGN ADMINISTRATIVE ALLOWANCE.

** THE AMOUNTS IDENTIFIED IN THE 'NET AMOUNT' COLUMN REPRESENTS THE COST PLUS 30% FOR KITS USED IN CONJUCTION WITH LABOR OPERATIONS V6010, V6011, V6012 AND V6013

DEALERS WILL AUTOMATICALLY RECEIVE THE CORRECT LABOR AND MATERIAL ALLOWANCE BASED ON THE LABOR OPERATION PERFORMED.

REFER TO THE CHEVROLET CLAIMS PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIMS SUBMISSION.

COPYRIGHT 1990 CHEVROLET MOTOR DIVISION. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.