SMU - SECTION 8A - A64 - A/C COMPRESSOR CONTROLS. GMC Truck S15 Pickup - 2WD 1994

For 1990-2009 cars

# SMU - SECTION 8A - A64 - A/C COMPRESSOR CONTROLS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8A-A64 - A/C COMPRESSOR CONTROLS - REVISED DIAGNOSTIC PROCEDURE - A/C COMPRESSOR CLUTCH DOES NOT ENGAGE

#### MODELS: 1994 CHEVROLET AND GMC TRUCK S/T MODELS WITH 4.3L ENGINES (VINS W, Z - RPOS L35, LB4)

THIS BULLETIN REVISES DIAGNOSTIC PROCEDURE, "A/C COMPRESSOR CLUTCH DOES NOT ENGAGE (4.3L ENGINE)," ON PAGE 8A-A64-8 AND 8A-A64-9 IN THE 1994 S/T SERVICE MANUAL BOOK 2 FINAL EDITION.

FIGURES: 0 ATTACHMENTS: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.