CAMPAIGN: PUSH-PULL HEADLIGHT SWITCH DEFECTIVE. GMC Truck S15 Pickup - 2WD 1985

For 1990-2009 cars

# CAMPAIGN: PUSH-PULL HEADLIGHT SWITCH DEFECTIVE

#### MODELS: 1985 S/Tl5 AND P25-35 MODEL LIGHT DUTY TRUCKS 1986 C/K, G-VAN, MEDIUM DUTY AND HEAVY DUTY MODEL TRUCKS

THE FOLLOWING INFORMATION SUPPLEMENTS THE "WARRANTY INFORMATION SECTION" OF CAMPAIGN BULLETIN 86-C-04. PLEASE UPDATE YOUR BULLETIN ACCORDINGLY.

Labor *Time Operation Allow- Trouble Number Description ance Code ------ ------------- ---- ---- V3260 Headlamp Switch S/T 0.9 Hr. 96 Inspect Only

V3262 Headlamp Switch S/T 0.9 Hr. 96 Inspect & Replace

(NOTE: TIME ALLOWANCE REVISED FOR S/T MODELS ONLY)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.