1989 PAINT CODES ALL TRUCKS. GMC Truck S15 Pickup - 4WD 1989

For 1990-2009 cars

# 1989 PAINT CODES ALL TRUCKS

THE FOLLOWING IS A LIST OF PAINT CODE NUMBERS FROM VARIOUS SUPPLIERS FOR THE 1989 MODEL YEAR. THESE COLORS CAN BE OBTAINED LOCALLY.

DUPONT REFINISH PAINTS ARE AVAILABLE IN:

. L - LUCITE(R) - ACRYLIC LACQUER

. A - CENTARI(R) - ACRYLIC ENAMEL

. D - DULUX(R) - ENAMEL

. 355S - FLEXIBLE ADDITIVE

. 1234 VINYL LACQUER - CHIP RESISTANT

#### IMPORTANT: VINYL RESIN MUST BE ADDED TO THE BASE COLOR WHEN PAINTING INTERIOR COMPONENTS.

DUPONT VINYL RESIN #304 - INSTRUMENT PANEL.

DUPONT VINYL RESIN #305 - ALL REMAINING INTERIOR PARTS EXCEPT SEATS.

DUPONT VINYL RESIN #306 - SEATS AND VINYL ROOFS.

WHEN ORDERING DUPONT PAINT, USE "L", "A", "D", 355S OR 1234 WITH THE APPROPRIATE DUPONT CODE.

DITZLER REFINISH PAINTS ARE AVAILABLE IN:

. DDL - DURACRYL - ACRYLIC LACQUER

. DBU - DELTRON - B/C

. DAR - DELSTAR - ACRYLIC ENAMEL

. DAU - DELTRON - ACRYLIC URETHANE

. UCV - VINYL COLORS

. DX-369 - FLEXATIVE - FLEXIBLE FINISHES

. DX-54 - ROADGUARD - ROAD ABRASION PROTECTION

WHEN ORDERING PPG PAINT, USE "DDL", "DBU", "DAR", "DAU", "UCV", "DX-369" OR "DX-54" WITH APPROPRIATE DITZLER CODE.

SHERWIN-WILLIAMS, ACME/ROGERS, AND MARTIN-SENOUR ARE AVAILABLE IN ACRYLIC LACQUER OR ACRYLIC ENAMEL.

S-W USE: PREFIX 34, J4 OR L10 FOR ACRYLIC LACQUER, PREFIX 35, J5 OR F10 FOR ACRYLIC ENAMEL.

ACME USE: PREFIX 84 FOR ACRYLIC LACQUER, PREFIX 85 FOR ACRYLIC ENAMEL.

ROGERS USE: PREFIX 94 FOR ACRYLIC LACQUER, PREFIX 95 FOR ACRYLIC ENAMEL.

MARTIN-SENOUR: JOBBER WILL INTERCHANGE NUMBER SHOWN WHEN ACRYLIC LACQUER IS NEEDED.

***1989 TRUCK EXTERIOR AND INTERIOR PAINT COLORS***

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1989 GMC TRUCK DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.