CONSOLE DOOR MODIFICATION IMPROVED APPEARANCE AND EFFORT. GMC Truck S15 Pickup - 4WD 1984

For 1990-2009 cars

# CONSOLE DOOR MODIFICATION IMPROVED APPEARANCE AND EFFORT

#### VEHICLES AFFECTED: 1983-85 S/T Pick-ups, Blazers and Jimmys Equipped RPO D55 Console ----------------------------------------

The seat separator console on 1983-85 S/T Pickups, Blazers and Jimmys can be modified to improve the appearance of the lid in the closed position and to allow less closure effort. These changes include the addition of a spring under the door middle attaching screw and a new spring at the door compartment stop.

#### SERVICE PROCEDURE

. Remove door from console body (see Figure No. 1).

. Install two washers, P/N 2077521, and spring, P/N 155445361 under the door centre attaching screw on the hinge side. The tab on the spring should point away from the hinge side of the console (see Figure No. 1).

. Discard existing spring at the door compartment stop and install spring, P/N 15544543 (see Figure No. 1).

. Reinstall console door.

#### PARTS INFORMATION

Part Number Description Quantity ----------- ----------- -------- 15544543 Spring 1 15544536 Spring 1 2077521 Washer 2

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.