ASSY PLANT IDENTIFICATION AND PAINT SUPPLIERS. GMC Truck S15 Pickup - 2WD 1991

For 1990-2009 cars

# ASSY PLANT IDENTIFICATION AND PAINT SUPPLIERS

#### SUBJECT: 1991 PAINT CODES, PAINT SUPPLIERS AND ASSEMBLY PLANT IDENTIFICATION

#### MODELS: ALL 1991 TRUCKS

The following is a list of paint code numbers from various suppliers for the 1991 model year. These colors can be obtained locally. BASF refinished paints are available in:

* A-Alphacryl * D-Diamont 88

* SO-Diamont Solo * 21-Glasurit-21 * 54-Glasurit-54 * S-Limco Select * L-Limco Supreme Gold * M-Miracryl * Super Max

Flexible Finishes

When spraying flexible plastic parts, use the following recommendations:

Elastifier additive 521-111 for Vinyl application when using Glasurit 54 and 21 lines.

891 Flex Agent for Vinyl Application when using Alphacryl, Miracryl, Diamont 88, and Supreme Gold.

DF-25 for Vinyl application when using Diamont Solo.

#### NOTE: When using a basecoatlclearcoat system only use the flex agent in the clearcoat application.

Stone Chip Protector

Glassohyd TM 1109-1240/6 Stone Chip Protector is a waterborne material based on a durable, flexible plastic dispersion as its bonding media. This prod- uct is versatile in application and may be easily applied by spray, brush, or roller. When Glassohyd TM is completely cured, the material is T resis- tant to water, gasoline, and oil. Glassohyd TM has excellent impact and corrosion resistance. Glasshoyd TM 1109-1240/6 Stone Chip Protector can be topcoated directly with 21-line or 54/94-line colors. DuPont refinished paints are available in:

-L-Lucite-Acrylic Lacquer -A-Centari-Acrylic Enamel -J-Cronar-Polyoxithane Enamel -K-Chromabase TM -35OS-Flexlar-Flexible Additive -310S-Black 1-2-3 Vinyl Lacquer -330S-White 1-2-3 Vinyl Lacquer -V-Lucite Vinyl

IMPORTANT Vinyl resin must be added to the base color when painting interior components.

DuPont vinyl resin #304-instrument panel

DuPont vinyl resin #305-all remaining interior parts except seats.

DuPont vinyl resin #306-seats and vinyl roofs.

When ordering Dupont paint, use "L", "A", "J", "K", "V", 350S or 1-2-3 White or 1-2-3 Black with the appropriate DuPont Code.

PPG (Ditzler) refinish paints are available in: - DDL - Duracryl - Acrylic Lacquer or Acrylic Basecoat/Clearcoat - DBU - Deltron - Basecoat/Clearcoat - DAR - Delstar - Acrylic enamel - DAU - Deltron - Acrylic Urethane - UCV - Vinyl colors - DX-369 - Flexative - Flexible Finishes - DX-54 - Roadguard - Road Abrasion Protection

When ordering PPG (Ditzler paint, use "DDL", "DBU", "DAR", "DAU", "UCV", "DX-54", "DX-369" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer, acrylic enamel, or acrylic urethane.

S-W use: prefix 34, J4 or L10 for acrylic lacquer, prefix 35, J5 or F10 for acrylic enamel, prefix UB for acrylic urethane in a basecoat/clearcoat system, prefix US for acrylic urethane in a single stage system

ACME use: prefix 84 for acrylic lacquer, prefix 85 for acrylic enamel, prefix PB for acrylic urethane in a basecoat/clearcoat system prefix PS for acrylic urethane in a single stage system.

Rogers Use: prefix 94 for acrylic lacquer, prefix 95 for acrylic enamel, prefix AU for acrylic urethane in a basecoat/clearcoat system prefix AS for acrylic urethane in a single stage system

Martin-Senour: Jobber will interchange number shown when acrylic lacquer is needed,

use prefix 98 for acrylic urethane as a pre-mix basecoat/clearcoat, use prefix 88 for acrylic urethane as a factory packaged basecoat/clearcoat,

use prefix 97 for acyrlic urethane as a pre-mix single stage system

use prefix 87 for acrylic urethane as a factory packaged single stage system.

1991 ASSEMBLY PLANT PAINT IDENTIFICATION

Attached is a current listing of the various assembly plants and their paint supplier. It should be noted, however, that paint suppliers are subject to change at any given time. Plant Paint Paint Type Assembly Plant Trucks Code Supplier ---------- ------------------------- ----- -------- Basecoat/Clearcoat Enamel Baltimore, Maryland B PPG (M-Vans)

Basecoat/Clearcoat Enamel Flint, Michigan F BASF (Suburban and Utility

High Solids Enamel Janesville, Wisconsin J Dupont (Med. Duty Truck and C/K)

High Solids Enamel Lordstown, Ohio (G-Van) 7 BASF

High Solids Enamel Moraine, Ohio (S/T-Truck) 2 BASF

Basecoat/Clearcoat Oshawa Truck Plant 1 ICI Waterborne (C/K Truck)

High Solids Enamel Pontiac-West, MI (S/T-Truck) 0 BASF

Basecoat Clearcoat Enamel Pontiac-East, MI (C/K Truck) E Dupont

Medium Solids Enamel Scarborough, Ontario (G-Van) 4 ICI

High Solids Enamel Shreveport, Louisiana 8 BASF (S-Truck)

Basecoat/Clearcoat Ft. Wayne, Indiana z Dupont (C/K Truck)

High Solids Enamel Flint, Michigan F BASF (R/V) F BASF

1991 TRUCK EXTERIOR COLORS

Sherwin- Paint Williams PPG BASF Glasurit Color Fisher Martin- Acme- DDL- Rinshed 54-21 Code Color Name W-Code DuPont Senour Rogers DAR Mason Line ----- ---------- ------ ------ ------ ------- --- ------ ------

10 White B/C 9225 B8796 36783 36783 4015 18121 GM-9225

12 White 5111 817 82-1208 F8W-2030 2185 1347 GM-5438 1492

15 Silver Metallic 8914 C8501 82-5915 34856 3796 15251 GM-7054 B/C

16 Warm Gray 9659 B9125 44149 44149 4314 21017 GM-9659 Metallic B/C

17 Slate Metallic 7468 B8235 82-5579 32377 3453 12866 GM-7023

19 Black 5118 99 8800 F10B-1738 9000/ Stdrd GM-1240 80-4080 9300 Pkg

22 Bahama Blue Met. 9656 B9126 44150 44150 4307 21018 GM-9656 B/C

23 Medium Blue 7154 B8041 82-5258 30527 3250 11500 GM-5481

24 Bright Blue 9222 B8894 38144 38144 4110 18120 GM-9222 Metallic

26 Pastel Blue 9662 B9128 44151 44151 4308 21019 GM-9662

27 Lt. Blue 9264 B8944 39337 39337 4146 19031 GM-9264 Metallic B/C

29 Dark Blue 7349 B8139 82-5448 31514 3362 12283 GM-5039

30 Med. Blue 9086 B9017 42478 42478 4238 20050 GM-9086 Metallic B/C

33 Light Mesa 9207 B8945 39338 39338 4152 19028 GM-9207 Brown B/C

34 Lt. Mesa Brown 9208 B8895 38145 38145 4107 18116 GM-9208 Met. B/C

37 Light Mesa Brown 9219 B8897 38147 38147 4111 18118 GM-9219

41 Black B/C 8555 99 82-5760 33756 9700 13572 54-1240

42 Sky Blue 9203 B8943 40381 40381 16813 19027 GM-9203

43 Seafoam Green 9663 B9129 44152 44152 4309 - GM-9663

44 Forest Green 7964 D8801 82-6024 35541 4114 15366 GM-7964 Metallic

46 Woodland Green 7156 B8046 82-5263 30530 3255 11505 GM-5482

47 Dark Blue 9095 B9019 42479 42479 4251 20052 GM-9095 Metallic

48 Dark Red 9096 B9020 42480 42480 4239 20053 GM-9096

50 White B/C 8624 B8550 82-5918 34851 3800 15255 GM-8624

51 Sedona Tan 8528 B8542 90-5857 34392 4310 15022 GM-8528

58 Lt. Sandstone 8865 B8792 36450 36450 4020 18111 GM-8865 Metallic B/C

61 Tan 8265 B8462 82-5799 34070 3686 14241 GM-1074

70 Red B/C 8832 B8793 36453 36453 4021 18115 GM-8332

71 Red Orange 7753 B8250 82-5586 32384 3463 12884 GM-3046

72 Bright Red 7475 B8241 82-5539 32097 3464 12885 GM-3047

74 Red B/C 9260 B8946 39339 39339 4154 19030 GM-9260

75 Red Metallic 8919 C8506 82-5945 34855 3804' 15259 GM-89191 B/C

77 Dk. Garnet Red 9154 B8742 36454 36454 4002' 21023 GM-9154 Met. B/C

78 Dark Maple 8800 B8632 90-6069 35366 3915 16117 GM-3091 Metallic

86 Wheatland Yellow 9418 B9044 43350 43350 21025 GM-9418

88 Tangier Orange 9417 B9045 43349 43349 21021 GM-9417

90 Gray Metallic 8798 B8629 82-6011 35367 3916 16118 GM-8798

94 Red Metallic B/C 9088 B9018 42481 42481 4240 20051 GM-9088

96 Silver Metallic 8867 B8795 36457 36457 4023 18112 GM-8867 B/C 97 Dk. Grey Metallic 9658 B9127 44153 44153 4313 21024 GM-9658 B/C

98 Black Sapphire 8863 B8745 36458 36458 4003 17118 GM-8863 Metallic B/C

1991 TRUCK INTERIOR COLORS

GM Gloss Fisher Sherwin Trim W-Code Martin- Williams Code Color Name Semi Flat Senour Acme Rogers --- ---------- --------- ------ ------ -----------

13AN Light Gray x 9653 44437 44438 x 44438 44437

13BN Medium Gray x 9654 44439 44439

13CN Dark Gray x 9655 44440 44440

18DN Dark x 7350 17113 34991 Charcoal x 16851 31901

19DN Black x 16918 33024 x 848 16615 J4-8677 92387

23DN Dark Blue X 7163 16742 30821

24CN Dark Blue x 9059 36478 36478 x 39838 39838

24DN Very Dark x 8576 17067 34598 Blue x 17075 34606

24EN Midnight x 9541 42600 42600 Blue x 42599 42599

47CN Dark Red x 9104 42602 42602 x 42601 42601

47DN Very Dark x 9253 42604 42604 Red x 42603 42603

60BN Medium Cognac x 9205 38394 38394 x 38393 38393

60CN Dark Cognac x 9099 38395 38395 x 38392 38392

60DN Very Dark x 9252 38391 38391 Cognac

69BN Medium Beige x 8248 16950 33715 x 16966 33770

69CN Medium Dark x 8280 17066 34597 Beige x 17074 34605

GM PPG PPG Vinyl (BASF) Trim DIA Interior Rinshed Code Color Name Code UCV Code Mason DuPont ----- ---------- ---- -------- ------- ------

13AN Light Gray 35203 2-1441 21029 C9109 35204

13BN Medium Gray 35205 2-1442 21027 C9110

13CN Dark Gray 35206 2-1443 21028 C9111

18DN Dark 33872 2-871 12730 C8575 Charcoal 33492 14030

19DN Black 9640 4401 9433 120 12812 C8535

23DN Dark Blue 15392 2-765 11595 C8002

24CN Dark Blue 16323 2-1276 17124 C8792 19021

24DN Very Dark 15886 2-1098 15080 C8539 Blue 16092 16045

24EN Midnight 16998 2-1396 20065 C9006 Blue 16999 20066

47CN Dark Red 73381 2-1394 20061 C9007 73380 20062

47DN Very Dark 73383 2-1395 20063 C9008 Red 73382 20064

60BN Medium Cognac 26281 2-1292 18055 C8808 - 19022

60CN Dark Cognac 26284 2-1315 18056 C8810 - 18057

60DN Very Dark 26285 2-1316 18059 C8819 Cognac

69BN Medium Beige 25313 2-1045 14006 C8446 20060

69CN Medium Dark 25514 2-1117 17120 C8554 Beige 25571 15065

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.