ENGINE COOLANT USAGE SPECIFICATIONS/RECOMMENDATIONS. GMC Truck S15 Pickup - 2WD 1982

For 1990-2009 cars

# ENGINE COOLANT USAGE SPECIFICATIONS/RECOMMENDATIONS

#### MODELS: 1982 LIGHT DUTY VEHICLES

General Motors has, in past model years, recommended use of ethylene glycol base anti-freeze that meets GM specification 1899-M. This recommendation has changed for 1982 vehicles which are factory filled with coolant which meets GM 1825-M specifications. It is required that any additions of coolant to these vehicles be done with GM 1825-M. This change was necessary due to the use of aluminum cylinder heads on some engines in 1982 which required a different formulation of anti-freeze to prevent corrosion. This anti-freeze is available from WDDGM in gallons and drums as P/N 1052752 and P/N 1052754.

This new coolant may be added to systems which contain anti-freeze meeting the GM 1899-M specification with no adverse effect, but it is recommended that when a complete draining of a cooling system is performed such as for engine repair, that it be refilled with one (1) source rather than mixing old anti-freeze with new as there may be slight differences in their chemical properties that could affect their overall performance.

As in the past, follow shop manual procedures for mixing anti-freeze to water to obtain the required protection level.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.