POP NOISE FROM WINDSHIELD PILLAR AREA (DIAG. INSTRUCT.). GMC Truck S15 Pickup - 4WD 1989

For 1990-2009 cars

# POP NOISE FROM WINDSHIELD PILLAR AREA (DIAG. INSTRUCT.)

#### SUBJECT: "POP" NOISE FROM WINDSHIELD PILLAR AREA (INFORMATION)

#### VEHICLES AFFECTED: 1983-93 "S/T" TRUCKS

REFERENCE COWL "POP" TAPPING NOISE BULLETIN, CORPORATE NUMBER 162001 R.'*

Owners of some 1983-1993 S/T Pickups and Utilities may comment on a cowl "pop" noise transmitted through the "A" pillar. It has been determined that sections other than the windshield cowl area may produce a sound which imitates cowl "pop".

PRIOR TO PERFORMING ANY CORRECTION FOR COWL "POP" TAPPING NOISES, VERIFY THE SOURCE OF THE NOISE(S) TO DETERMINE IF IT IS A VALID COWL "POP" CONDITION.

Possible noise areas to check are:

0 Instrument panel "itch"/noise.

0 Loose door lock rods.

0 Loose wires/harnesses contacting the wall of the engine/passenger compartment (cowl).

0 A lack of door hinge lubrication.

0 An Electronic Control Module (ECM) bracket "itch".

0 An ash tray rattle.

0 An air vent squeak.

0 Hood hinge "flutter"/rattle.

#### INFORMATION:

----------- 1. INSTRUMENT PANEL (I/P) "ITCH"/NOISE sound at the front edge of the I/P may occur if the I/P pad rubs against the cowl/dash support panel.

Refer to "Instrument Panel Pad to Cowl Panel "Itch" Noise" Bulletin Corporate Number 261610."

2. LOOSE DOOR LOCK RODS may vibrate during vehicle operation creating a rattle type noise.

Refer to "Front Door Lock Rod Rattle" Bulletin Corporate Number 161603."

3. THE ELECTRONIC CONTROL MODULE (ECM) WIRING HARNESS CLIP may not be properly attached at the transmission bellhousing bolt allowing contact with the floor pan/front of dash area. This sound may be amplified by the HVAC ductwork.

4. LOOSE WIRES/HARNESSES may be tapping against the engine/passenger compartment wall (cowl).

5. LACK OF DOOR HINGE LUBRICATION - Insufficient lubrication may create a binding/squeaking condition.

6. AN ECM BRACKET "ITCH" sound may occur if the ECM moves within its mounting bracket.

7. AN ASH TRAY BRACKET RATTLE coming from the ash tray or radio area of the instrument panel may occur if the bracket is loose and vibrating against the I/P.

8. AN AIR VENT "ITCH" may occur if the louvered vent and A/C duct rub together.

9. HOOD "FLUTTER"/RATTLE may occur if there is movement in the hood hinge attachment to the truck frame. Sound may accompany the hood movement.

Refer to Bulletin Corporate Number 061006."

#### BULLETIN REFERENCES:

Corporate Ref. 162001 R

General Motors of Canada 91-2-235 Chevrolet Division 91-351-10 Oldsmobile Division 91-T-167 GMC Truck Division 91-2-122

Corporate Ref. 261610

General Motors of Canada 93-10-113 Chevrolet Division 92-286-10 Oldsmobile Division 92-T-128 GMC Truck Division 92-10-130

Corporate Ref. 161603

General Motors of Canada 91-2-243 Chevrolet Division 91-406-10 Oldsmobile Division 91 -T- 1 94 GMC Truck Division 91-10-144

Corporate Ref. 061006

General Motors of Canada 91-2-108 Chevrolet Division 91-181-10 GMC Truck Division 91-10-20

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.