CREAK/SQUEAK IN 'B' PILLER MODIFY MOUNT BELOW 'B' PILLER. GMC Truck S15 Pickup - 4WD 1991

For 1990-2009 cars

# CREAK/SQUEAK IN 'B' PILLER MODIFY MOUNT BELOW 'B' PILLER

#### SUBJECT: CREAK/SQUEAK NOISE IN "B" PILLAR (APPLY LOCKING COMPOUND AND RETORQUE)

#### VEHICLES AFFECTED: 1991 S/T 2 AND 4 DOOR UTILITY VEHICLES

Some 1991 S/T utility vehicles may experience a creak or squeak in the "B" pillar post that is located directly behind the front door. This condition is caused by movement between the floor of the cab and the number two body mount located directly under the "B" pillar and may occur on either or both sides of the vehicle.

To correct the condition, use the following procedure:

1. Remove the #2 body mount bolt.

2. Raise the body off the mount to obtain clearance between the floor and the top of the body mount.

3. Cut a 101mm x 101mm (4 inch x 4 inch) square of 1/32" thick teflon (obtain locally) and drill a 15mm (5/8") hole through the centre Insert this between the floor pan and the body mount and lower the body.

4. Clean the body mount bolt and apply Loctite 242 thread locking compound (GM P/N (12345382) or equivalent to the body mount bolt and retorque to 70-80 N.m. (52-59 ft.lbs.).

#### Notice: Concern exists that some insulating materials may compress over time resulting in a loss of torque to the body mount bolt. For this reason, teflon, 1/32 inch thick, and the thread locking compound on the bolt are being specified.

An alternative to preferred teflon material that can be found in most truck dealerships consists of using three washer pump shields P/N 22063244 .

Using this method, cut three sheets to size and locate a 15mm (5/8 inch) hole in the centre of each sheet. Place the three sheets between the floor pan and the mount and lower the body on the mount. Clean the body mount bolt and apply thread locking compound as described above and retorque bolt to 70-80 N.m. (52-59 ft.lbs.)

#### SERVICE PARTS INFORMATION

Part Number Description --------------- --------------------------------- 12345382 Loctite 242 thread locking compound or equivalent

22063244 Washer pump shields or equivalent teflon material

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.