Range Selector Lever Cable Bracket Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner duct. Refer to Engine Controls.
2. Remove the automatic transaxle range selector lever cable from the automatic transaxle range selector lever. Refer to Range Selector Lever Cable Replacement .
3. Remove the automatic transaxle range selector lever cable from the bracket. Refer to Range Selector Lever Cable Replacement .
4. Remove the automatic transaxle range selector lever cable bracket bolts.
5. Remove the automatic transaxle range selector lever cable bracket.

### Installation Procedure

1. Install the automatic transaxle range selector lever cable bracket.
2. Install the automatic transaxle range selector lever cable bracket bolts.

Tighten
Tighten the automatic transaxle range selector lever cable bracket bolts to 25 N·m (18 lb ft). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Install the automatic transaxle range selector lever cable to the bracket. Refer to Range Selector Lever Cable Replacement .
4. Install the automatic transaxle range selector lever cable to the automatic transaxle range selector lever. Refer to Range Selector Lever Cable Replacement .
5. Adjust the automatic transaxle range selector lever cable if necessary. Refer to Range Selector Lever Cable Adjustment .
6. Install the air cleaner duct. Refer to Engine Controls.