Electronic Brake Control Relay Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster panel. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
2. Release the electronic brake control relay (2) from the EBCM/EBTCM bracket (1).
3. Remove the electronic brake control relay connector.

### Installation Procedure

1. Install the electronic brake control relay electrical connector.
2. Slide the electronic brake control relay (2) into the EBCM/EBTCM bracket (1) until the electronic brake control relay is secure.
3. Install the knee bolster panel. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.