Wiring Harness Shield Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the vacuum modulator and wiring harness shield nut.
2. Remove the vacuum modulator and wiring harness shield.

### Installation Procedure

1. Install the vacuum modulator and wiring harness shield.
2. Install the vacuum modulator and wiring harness shield nut.

Tighten
Tighten the vacuum modulator and wiring harness shield nut to 17 N·m (13 lb ft). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.