Rear Seat Adjuster Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the seat. Refer to Rear Seat Replacement .
2. Remove the seat riser. Refer to Rear Seat Riser Replacement .
3. Remove the seat adjuster bolts.
4. Remove the seat adjuster from the seat.

### Installation Procedure

1. Install the seat adjuster to the seat.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the seat adjuster bolts.

Tighten
Tighten the bolts to 32 N·m (24 lb ft).

3. Install the seat riser. Refer to Rear Seat Riser Replacement .
4. Install the seat. Refer to Rear Seat Replacement .